V­­­F is the forward voltage. It refers to minimum voltage that diode needs to allow current flow

VR is reverse breakdown voltage. It shows the maximum reverse voltage that the diode can hold. This parameter mostly depends on the doping and semiconductor characteristics. There is also another term called non repetitive peak reverse voltage VRSM. It also refers to the maximum reverse voltage provided that it is not repetitive.